ENTER '4' TO TURN ON THE CASSETTE RECORDER MOTOR                                
? 4                                                                             
MOTOR ON                                                                        
ENTER '0' TO TURN THE MOTOR OFF                                                 
? 0                                                                             
MOTOR OFF                                                                       
