What attenuator do you want, TEE, PI or MINIMUM LOSS..? PI                      
                                                                                
What is the input impedance...? 75                                              
                                                                                
What is the output impedance..? 50                                              
                                                                                
What is the required loss (in dB)...? 3                                         
Specified loss is too low..adjusting to....                                     
MINIMUM LOSS PAD DESIGN                                                         
                                                                                
Pad for Z1 > Z2                                                                 
                                                                                
----R1--------                                                                  
         |                                                                      
         R2                                                                     
         |                                                                      
--------------                                                                  
Source Impedance= 75 ,Terminating Impedance= 50                                 
R1=, 43.3013 ,R2= 86.6025                                                       
Loss (dB)= 5.71946                                                              
                                                                                
                                                                                
What attenuator do you want, TEE, PI or MINIMUM LOSS..? TEE                     
                                                                                
What is the input impedance...? 75                                              
                                                                                
What is the output impedance..? 50                                              
                                                                                
What is the required loss (in dB)...? 3                                         
Specified loss is too low..adjusting to....                                     
MINIMUM LOSS PAD DESIGN                                                         
                                                                                
Pad for Z1 > Z2                                                                 
                                                                                
----R1--------                                                                  
         |                                                                      
         R2                                                                     
         |                                                                      
--------------                                                                  
Source Impedance= 75 ,Terminating Impedance= 50                                 
R1=, 43.3013 ,R2= 86.6025                                                       
Loss (dB)= 5.71946                                                              
                                                                                
                                                                                
What attenuator do you want, TEE, PI or MINIMUM LOSS..? MIN                     
                                                                                
What is the input impedance...? 75                                              
                                                                                
What is the output impedance..? 50                                              
MINIMUM LOSS PAD DESIGN                                                         
                                                                                
Pad for Z1 > Z2                                                                 
                                                                                
----R1--------                                                                  
         |                                                                      
         R2                                                                     
         |                                                                      
--------------                                                                  
Source Impedance= 75 ,Terminating Impedance= 50                                 
R1=, 43.3013 ,R2= 86.6025                                                       
Loss (dB)= 5.71946                                                              
                                                                                
                                                                                
What attenuator do you want, TEE, PI or MINIMUM LOSS..? QUIT                    
