10 REM 'NOFLOW' TEST PROGRAM
20 PRINT "THE FIRST THREE LINES OF THIS PROGRAM"
30 NOFLOW
40 PRINT "ARE PRINTED WITH THE TRACE TURNED ON."
50 PRINT "THIS LINE IS PRINTED WITH THE TRACE TURNED OFF."
99 END
