Digital Mars Compiler Version 8.42n
Copyright (C) Digital Mars 2000-2004.  All Rights Reserved.
Written by Walter Bright  www.digitalmars.com/ctg/sc.html
DMC is a one-step program to compile and link C++, C and ASM files.
Usage ([] means optional, ... means zero or more):

	DMC file... [flags...] [@respfile] 

file...		.CPP, .C or .ASM source, .OBJ object or .LIB library file name
@respfile...	pick up arguments from response file or environment variable
flags...	one of the following:
-a[1|2|4|8] alignment of struct members	-A  strict ANSI C/C++
-Aa enable new[] and delete[]		-Ab enable bool
-Ae enable exception handling		-Ar enable RTTI
-B[e|f|g|j] message language: English, French, German, Japanese
-c  skip the link, do compile only	-cpp  source files are C++
-cod  generate .cod (assembly) file	-C  no inline function expansion
-d  generate .dep (make dependency) file
-D  #define DEBUG 1			-Dmacro[=text]  define macro
-e  show results of preprocessor	-EC do not elide comments
-EL #line directives not output		-f  IEEE 754 inline 8087 code
-fd work around FDIV problem		-ff fast inline 8087 code
-g  generate debug info
-gf disable debug info optimization	-gg make static functions global
-gh symbol info for globals		-gl debug line numbers only
-gp generate pointer validations	-gs debug symbol info only
-gt generate trace prolog/epilog	-GTnnnn set data threshold to nnnn
-H  use precompiled headers (ph)	-HDdirectory  use ph from directory
-HF[filename]  generate ph to filename	-HHfilename  read ph from filename
-HIfilename   #include "filename"	-HO include files only once
-HS only search -I directories          -HX automatic precompiled headers

-Ipath	#include file search path	-j[0|1|2]  Asian language characters
    0: Japanese 1: Taiwanese and Chinese 2: Korean
-Jm relaxed type checking		-Ju char==unsigned char
-Jb no empty base class optimization    -J  chars are unsigned
-l[listfile]  generate list file	-L  using non-Digital Mars linker
-Llink  specify linker to use		-L/switch  pass /switch to linker
-Masm   specify assembler to use	-M/switch  pass /switch to assembler
-m[tsmclvfnrpxz][do][w][u] set memory model
    s: small code and data		m: large code, small data
    c: small code, large data		l: large code and data
    v: VCM				r: Rational 16 bit DOS Extender
    p: Pharlap 32 bit DOS Extender	x: DOSX 32 bit DOS Extender
    z: ZPM 16 bit DOS Extender		f: OS/2 2.0 32 bit
    t: .COM file			n: Windows 32s/95/98/NT/2000/ME/XP
    d: DOS 16 bit			o: OS/2 16 bit
    w: SS != DS				u: reload DS
-Nc function level linking		-NL no default library
-Ns place expr strings in code seg	-NS new code seg for each function
-NTname  set code segment name		-NV vtables in far data
-o[-+flag]  run optimizer with flag	-ooutput  output filename
-p  turn off autoprototyping		-P  default to pascal linkage
-Pz default to stdcall linkage		-r  strict prototyping
-R  put switch tables in code seg	-s  stack overflow checking
-S  always generate stack frame		-u  suppress predefined macros
-v[0|1|2] verbose compile		-w  suppress all warnings
-wc warn on C style casts
-wn suppress warning number n		-wx treat warnings as errors
-W{0123ADabdefmrstuvwx-+}  Windows prolog/epilog
	-WA  Windows EXE
	-WD  Windows DLL
-x  turn off error maximum		-XD instantiate templates
-XItemp<type>  instantiate template class temp<type>
-XIfunc(type)  instantiate template function func(type)
-[0|2|3|4|5|6]  8088/286/386/486/Pentium/P6 code
	      for (l = l->OtherLine; l->cmdnum != C_END_IF; l = l->OtherLine);
	                                                                    ^
bwbasic.c(2440) : Warning 7: possible extraneous ';'
		   l = l->OtherLine);
		                   ^
bwbasic.c(2446) : Warning 7: possible extraneous ';'
      for (x = x->OtherLine; x->cmdnum != C_END_IF; x = x->OtherLine);
                                                                    ^
bwb_cmd.c(6092) : Warning 7: possible extraneous ';'
      for (x = x->OtherLine; x->cmdnum != C_END_SELECT; x = x->OtherLine);
                                                                        ^
bwb_cmd.c(6097) : Warning 7: possible extraneous ';'
  for (l = l->OtherLine; l->OtherLine != NULL; l = l->OtherLine);
                                                               ^
bwb_cnd.c(581) : Warning 7: possible extraneous ';'
  for (l = l->OtherLine; l->OtherLine != NULL; l = l->OtherLine);
                                                               ^
bwb_cnd.c(599) : Warning 7: possible extraneous ';'
  for (l = l->OtherLine; l->OtherLine != NULL; l = l->OtherLine);
                                                               ^
bwb_cnd.c(899) : Warning 7: possible extraneous ';'
  for (l = l->OtherLine; l->OtherLine != NULL; l = l->OtherLine);
                                                               ^
bwb_cnd.c(917) : Warning 7: possible extraneous ';'
	  for (m = 0; m < n && buff_skip_char (buffer, &q, T->Name[m]); m++);
	                                                                   ^
bwb_exp.c(1881) : Warning 7: possible extraneous ';'
      for (; x->cmdnum != C_DATA && x != My->EndMarker; x = x->next);
                                                                   ^
bwb_inp.c(945) : Warning 7: possible extraneous ';'
	 x = x->next);
	            ^
bwb_stc.c(1358) : Warning 7: possible extraneous ';'
    for (argn = argv; argn->next != NULL; argn = argn->next);
                                                           ^
bwb_stc.c(1389) : Warning 7: possible extraneous ';'
	while (line_skip_seperator (l));
	                              ^
bwb_var.c(113) : Warning 7: possible extraneous ';'
bwbasic.c:
bwb_cmd.c:
bwb_cnd.c:
bwb_dio.c:
bwb_exp.c:
bwb_fnc.c:
bwb_inp.c:
bwb_int.c:
bwb_prn.c:
bwb_stc.c:
bwb_str.c:
bwb_tbl.c:
bwb_var.c:
bwd_cmd.c:
bwd_fun.c:
bwx_tty.c:
link cx+bwbasic+bwb_cmd+bwb_cnd+bwb_dio+bwb_exp+bwb_fnc+bwb_inp+bwb_int+bwb_prn+bwb_stc+bwb_str+bwb_tbl+bwb_var+bwd_cmd+bwd_fun+bwx_tty,BWBASIC.EXE,,X32/noi;

